Top of Form

First Name

Your First Name

Surname

Your Last Name

Beach Location

Site Location

Membership Number

Membership Number

Valid Email Address

Your Email Address

Date You Are Sailing

Select a date

**Chassis & Steering**

Wheel bearings rotate freely without excessive play.

Satisfactory

Defective

Not Applicable

Tyres show no signs of cracking, wall damage or canvas breakthrough.

Satisfactory

Defective

Not Applicable

All axle bolts and wheel retaining nuts are tight and wheel retaining clips, where required are in place.

Satisfactory

Defective

Not Applicable

Steering mechanism moves smoothly and without excessive play in links and bushes.

Satisfactory

Defective

Not Applicable

Steering rotation has sufficient travel lock to lock and cannot over-extend and remain locked in one position.

Satisfactory

Defective

Not Applicable

Steering shackles, where fitted, must be wire locked (C3).

Satisfactory

Defective

Not Applicable

Steering cables, where fitted must meet class specifications (C3).

Satisfactory

Defective

Not Applicable

Steering cables must be free from visual defects, broken strands (cables)

Satisfactory

Defective

Not Applicable

Steering cables must be routed to avoid chafe, kinks or excessive friction.

Satisfactory

Defective

Not Applicable

Cable tensioners, where fitted, must have a locking mechanism to prevent loosening (C3).

Satisfactory

Defective

Not Applicable

Chassis / monocoque is free from visible defects.

Satisfactory

Defective

Not Applicable

Any separate seat or foot pan or steering bar stirrup is secure and free from visible defects.

Satisfactory

Defective

Not Applicable

Sand brake where fitted operates and returns freely.

Satisfactory

Defective

Not Applicable

Mandatory Sand brake is fitted to C3, operates and returns freely.

Satisfactory

Defective

Not Applicable

On Blokarts and X-Sails all quick release levers and Spring retainers are in place and correctly tensioned.

Satisfactory

Defective

Not Applicable

**Mast & Mast Support**

Mast step shows no visible defect.

Satisfactory

Defective

Not Applicable

Mast stays and cables, when used are secure and meet Class specifications where applicable.

Satisfactory

Defective

Not Applicable

**Pulley and Sail Control**

All pulleys and rope guides run freely and ratchet blocks, where fitted are correctly aligned and allow the sheet to be released when necessary

Satisfactory

Defective

Not Applicable

Sheet is in good condition without fraying or swelling that might impair free movement.

Satisfactory

Defective

Not Applicable

Sheet and boom move freely.

Satisfactory

Defective

Not Applicable

The pilot has a suitable helmet free from defects. C3 meets BS 6658:1985

Satisfactory

Defective

Not Applicable

If you have answered defective to any of the above, please rectify the fault and report here what you have done ie: changed bearings. PLEASE NOTE: If you do not rectify any defective errors, your insurance will be invalid

Question

Submit

Bottom of Form